Just tap water is safe to eat

Gunsan k-water quality test results

( March, 2019 )

Yongdam process water purification treatment process through the scientific safe and clean water

Water Source

【 Youngdam Front view 】

Water Treatment Process

intake Water  Place

Disinfection Place

Disinfection Place

Filtration Place

Sedimentation Place

Water supply

Home

Aggregation Place

Start Place

Mixed Place

Water treatment plant and reservoir inflow

K-water produces a monthly water quality test results in water suitable for drinking     water as the water is received is determined

○ Water sampling date : March 5, 2019

○ Test period :  March 5, 2019  ~   March 27, 2019

No.	Test items	water standards	Test results		No.	Test items	water standards	Test results
			Water Plant	Gunsan water				Water Plant	Gunsan water
1	Bacteria	100CFU/㎖Less	0	0	31	1,2dibromo-3-chloropropane	0.003㎎/ℓLess	ND	ND
2	Total Coliforms	ND/100㎖	ND	ND	32	1,4-dioxane	0.05㎎/ℓLess	ND	ND
3	E.coli	ND/100㎖	ND	ND	33	Residual chlorine	4.0㎎/ℓLess	0.74	0.47
4	Pb	0.01㎎/ℓLess	ND	ND	34	Trihalomethanes	0.1㎎/ℓLess	0.029	0.036
5	F	1.5㎎/ℓLess	ND	ND	35	chloroform	0.08㎎/ℓLess	0.024	0.030
6	As	0.01㎎/ℓLess	ND	ND	36	bromodichloromethane	0.03㎎/ℓLess	0.005	0.006
7	Se	0.01㎎/ℓLess	ND	ND	37	dibromochloromethane	0.1㎎/ℓLess	ND	ND
8	Hg	0.001㎎/ℓLess	ND	ND	38	chloralhydrate	0.03㎎/ℓLess	0.0012	0.0025
9	CN	0.01㎎/ℓLess	ND	ND	39	Dibromoacetonitrile	0.1㎎/ℓLess	ND	ND
10	Cr	0.05㎎/ℓLess	ND	ND	40	Dichloroacetonitrile	0.09㎎/ℓLess	0.0010	0.0017
11	NH3-N	0.5㎎/ℓLess	ND	ND	41	Trichloroacetonitrile	0.004㎎/ℓLess	ND	ND
12	NO3-N	10㎎/ℓLess	1.3	1.3	42	Haloaceticacid	0.1㎎/ℓLess	0.018	0.023
13	Cd	0.005㎎/ℓLess	ND	ND	43	Formaldehyde	0.5㎎/ℓLess	ND	ND
14	B	1.0㎎/ℓLess	0.01	ND	44	Hardness	300㎎/ℓLess	35	34
15	Bromate	0.01㎎/ℓLess	ND	ND	45	Donsumption of ptas sium permanganate	10㎎/ℓLess	2.3	2.1
16	Phenol	0.005㎎/ℓLess	ND	ND	46	Smell	only the raw smell of disinfection	None	None
17	Diazinon	0.02㎎/ℓLess	ND	ND	47	Taste	only the raw taste of disinfection	None	None
18	Parathion	0.06㎎/ℓLess	ND	ND	48	Cu	1㎎/ℓLess	ND	ND
19	Fenitrothion	0.04㎎/ℓLess	ND	ND	49	Color	5 Less	ND	ND
20	Carbaryl	0.07㎎/ℓLess	ND	ND	50	ABS	0.5㎎/ℓLess	ND	ND
21	1.1.1-Trichloroethane	0.1㎎/ℓLess	ND	ND	51	PH	5.8 ~ 8.5	7.1	7.1
22	Tertachloroethylene	0.01㎎/ℓLess	ND	ND	52	Zn	3㎎/ℓLess	ND	ND
23	Trichloroethylene	0.03㎎/ℓLess	ND	ND	53	Cl-	250㎎/ℓLess	12.1	12.4
24	Dichloromethane	0.02㎎/ℓLess	ND	ND	54	Residue on evaporation	500㎎/ℓLess	83	46
25	Benzene	0.01㎎/ℓLess	ND	ND	55	Fe	0.3㎎/ℓLess	ND	ND
26	Toluene	0.7㎎/ℓLess	ND	ND	56	Mn	0.05㎎/ℓLess	ND	ND
27	Ethylbenzene	0.3㎎/ℓLess	ND	ND	57	Turbidity	0.5NTULess	0.05	0.06
28	Xylene	0.5㎎/ℓLess	ND	ND	58	SO42-	200㎎/ℓLess	6	6
29	1.1-Dichloroethylene	0.03㎎/ℓLess	ND	ND	59	Al	0.2㎎/ℓLess	ND	ND
30	Tetrchlorocarbon	0.002㎎/ℓLess	ND	ND	Test results			Suitable	Suitable
Test results			Suitable	Suitable

Plumbing Faucet

Every month 41 locations in tap water safety test results

○ Water sampling test : March 4, 2019 ~ March 6, 2019

○ Test period : March 4, 2019 ~ March 19, 2019

▶ Faucet

Bacteria (100CFU/㎖Less)		Totalcoliforms (ND/100㎖)		E.coli (ND/100㎖)		Residual chlorine (4.0mg/ℓLESS)
Average	Max	Average	Max	Average	Max	Average	Max
0	0	ND	ND	ND	ND	0.21	0.28

▶ After passing through a water tank faucet

Bacteria (100CFU/㎖Less)		Totalcoliforms (ND/100㎖)		E.coli (ND/100㎖)		Residual chlorine (4.0mg/ℓLESS)
Average	Max	Average	Max	Average	Max	Average	Max
0	0	ND	ND	ND	ND	0.18	0.26

▶ The end of the faucet

구 분	Bacteria (100CFU/mℓLess)	Totalcoliforms (ND/100mL)	E.coli (ND/100mL)	Residual chlorine (4.0 mg/ℓLess)	Fe (0.3 mg/ℓLess)	Cu (1 mg/ℓLess)	Zn (3 mg/ℓLess)	Mn (0.3 mg/ℓLess)	NH3-N (0.5 mg/ℓLess)	Cl- (250mg/ℓLess)
Average value	0	ND	ND	0.20	ND	ND	0.003	ND	ND	9.6
Maximum value	0	ND	ND	0.22	ND	ND	0.005	ND	ND	9.7

Small Water Supply

○ Facilities : 6 facilities (each on Gwanli island, Bangchuk island, Eocheong island, Yeon island, Gaeya island, Bian island )

○ Water sampling period : March 11 ~ March 29, 2019

○ Test period : March 11 ~ April 4, 2019

○ Test items  : 13 items for filtered water

○ Test result : Suitable

Small Water Supply Facilities

○ Facilities : 4 facilities (each on Myeong island, Mal island, Duri island, Juk island)

○ Water sampling period : March 14 ~ April 8, 2019

○ Test period : March 14 ~ April 9 , 2019

○ Test items  : 13 items  for filtered water

○ Test result : Suitable

Contact water quality

♣ Counter complaints : Gunsan city water service section

♣ Complaints Phone : No area code 120times

☎ Adminstration 454-5352 Charge 454-5362

Water Mangement 454-5382 Water sector 454-5392, 5402, 5422

Monthly water quality test results reveal the homepage